|  |  |
| --- | --- |
| VOLTAGE | SITUATION |
| <0.86V | Completely dead |
| 0.86V～1.16V | Nearly dead |
| 1.16V～1.33V | Available for low-power appliances |
| >1.33V | Available for all appliances |